
**Jurassic World: Fallen Kingdom Chevy S10 Maintenance Truck**







**General Information:**

* 1998-2004 Chevy S10 Pickup
  + Base model
  + Regular cab/short bed
  + Front bumper and fleetside rear bumper - black

1994-1997 Alternative Option with front and back end conversion (body is virtually identical with part swapping)

* 1994-1997 Chevy S10 Pickup
  + Base model
  + Regular cab/short bed

1998-2004 model parts required for front/rear end conversion of ’94-’07 models

**Front End**

* + Radiator support - GM 15009394
  + Grille (dark grey plastic) - GM 19180339
  + Grille retainers (11 needed) - GM 15002520
  + Headlights (driver/passenger) - GM 16526218
  + Headlight retaining clips (2 sets) - GM 15734237
  + Turn signals (without fog lamp) - GM 15098267 and 15098268
  + Low beam pigtails - Dorman Headlight Socket 85813
  + High beam pigtails - Dorman Headlight Socket 85812
  + Front bumper - GM 1002367
  + Front valence - GM 1092162

**Rear End**

* + Full Pickup fleetside bumper kit (black)(bumper, pads, brackets, lights, etc.) – Amazon, etc.

**Forum threads about ’94-’97 to ’98-04 conversions:**

<https://www.s10forum.com/threads/94-97-to-98-light-conversion.460218/>

<https://www.s10forum.com/threads/how-to-convert-your-94-97-front-clip-to-98-s-10.208724/>

**Body:**

Paint: Light Metallic Pewter - GM paint code WA382E

**Interior:**

* Charcoal black cloth seats
* Black dash, inner door panels and flooring.



**Wheels:**

* Base steel rims - part # 05030 (GM STL05030U20)
* Chevy black lug nut covers
* Tires – light duty truck/SUV tires (all black/no whitewalls)

**Roll Bars**

* Custom fabricated dual tube roll bars/headache rack

**Decals:**

* Door decals:
  + 2 x 11” Jurassic World emblem

****

* + 2 x “MAINTENANCE” - 3” tall letters with 0.5 “ separating each character
* Truck bed decals:
  + ****2 x your vehicle number - 6.5” tall with 0.5” separating each character
* Use USAAF font for all lettering

